Author: EC

Bleed Area: .125” minimum Safe Margin Area: .075” Design Area: innermost margin